#### To start GNURadio Companion ####
gnuradio-companion

#### To read the hardwaregain attribute of the voltage0 INPUT channel of the ad9361-phy control device ####

iio_attr -u ip:pluto.local -c -i ad9361-phy voltage0 hardwaregain


#### To write the hardwaregain attribute of the voltage0 INPUT channel of the ad9361-phy control device ####

iio_attr -u ip:pluto.local -c -i ad9361-phy voltage0 hardwaregain 5


